Noitom Hi5 Unity SDK: Class Members

| Noitom Hi5 Unity SDK Hi5_Unity_SDK_API_1_0_0_655_17 The SDK for Using Noitom Hi5 Glove in Unity Engine.

Here is a list of all documented class members with links to the class documentation for each member:

### - b -

- BindInfo : HI5.HI5_BindInfoManager

### - c -

- CheckDeviceBinded() : HI5.HI5_BindInfoManager
- Connect() : HI5.HI5_Manager

### - d -

- DefaultPath : HI5.HI5_BindInfoManager , HI5.HI5_Calibration
- DisConnect() : HI5.HI5_Manager

### - e -

- EnableBothGlovesVibration() : HI5.HI5_Manager
- EnableLeftVibration() : HI5.HI5_Manager
- EnableRightVibration() : HI5.HI5_Manager

### - g -

- GetBindedTrackedObjectSerialNumber() : HI5.HI5_Calibration
- GetBindedTrackedObjectType() : HI5.HI5_Calibration
- GetCalibrationProgress() : HI5.HI5_Calibration
- GetGloveStatus() : HI5.HI5_Manager
- GetHI5Source() : HI5.HI5_Manager
- GetMagneticState() : HI5.HI5_GloveStatus
- GetPowerLevel() : HI5.HI5_GloveStatus
- GetReceivedPosition() : HI5.HI5_Source
- GetReceivedRotation() : HI5.HI5_Source

### - i -

- IsCalibratingBPose : HI5.HI5_Calibration
- IsCalibratingPPose : HI5.HI5_Calibration
- IsCalibrationBposSuccess : HI5.HI5_GloveStatus
- IsConnected : HI5.HI5_Manager
- IsDongleAvailable() : HI5.HI5_Manager
- IsGloveAvailable() : HI5.HI5_GloveStatus
- IsGloveBinded() : HI5.HI5_BindInfoManager
- isGloveBPosSuccess() : HI5.HI5_GloveStatus
- IsLeftGloveAvailable : HI5.HI5_GloveStatus
- IsLeftGloveBinded : HI5.HI5_BindInfoManager
- IsRightGloveAvailable : HI5.HI5_GloveStatus
- IsRightGloveBinded : HI5.HI5_BindInfoManager
- IsVisibleLog : Hi5_Log

### - l -

- L_BonePos : HI5.HI5_Source
- L_BoneRot : HI5.HI5_Source
- LeftID : HI5.HI5_BindInfoManager
- LeftMagneticStatus : HI5.HI5_GloveStatus
- LeftOffset : HI5.HI5_Manager
- LeftPower : HI5.HI5_GloveStatus
- LoadCalibrationData() : HI5.HI5_Calibration
- LoadItems() : HI5.HI5_BindInfoManager

### - m -

- MainThreadUpdate() : HI5.HI5_GloveStatus

### - o -

- OnCalibrationComplete : HI5.HI5_Calibration
- OnStatusChanged : HI5.HI5_GloveStatus

### - p -

- PushOpticalData() : HI5.HI5_DataTransform

### - r -

- R_BonePos : HI5.HI5_Source
- R_BoneRot : HI5.HI5_Source
- ResetCalibration() : HI5.HI5_Calibration
- RightID : HI5.HI5_BindInfoManager
- RightMagneticStatus : HI5.HI5_GloveStatus
- RightOffset : HI5.HI5_Manager
- RightPower : HI5.HI5_GloveStatus

### - s -

- SaveCalibrationData() : HI5.HI5_Calibration
- SaveItems() : HI5.HI5_BindInfoManager
- SetTrackedObjectBindState() : HI5.HI5_Calibration
- StartCalibration() : HI5.HI5_Calibration
- Status : HI5.HI5_GloveStatus

### - t -

- ToUnityEulerAngles() : HI5.HI5_DataTransform
- ToUnityPosition() : HI5.HI5_DataTransform